polycarboxylate ether PCE powder concrete additive concrete admixture

polycarboxylate ether PCE powder concrete additive concrete admixture is a new type of environmental protection superplasticizer. The product is concentrated product, the best water reduction rate is high, slump retention ability is strong, alkali content is low, strength gain rate is high.

At the same time, it can also improve the plastic index of fresh concrete, so as to improve the pumping performance of concrete in construction. It can be widely used in premix of ordinary concrete, shotcrete and high strength and durability concrete. Especially! It has excellent performance and can be used in high strength and durability concrete.

Product technical performance
1. Special molecular structure and special branch structure design, used for hydrolysis reaction of fresh mixed concrete. By adjusting the branch structure, the hydrolysis rate can be adjusted within the effective time to achieve selective protection effect.
2. Slow release: this product is mixed into concrete, slowly hydrolyze, release carboxylic acid group, achieve long-term dispersion effect, achieve ideal preservation effect.
3. High strength increase rate, adding the product of concrete does not change the setting time, to overcome the general retarder concrete final setting time is too long, early strength development is too slow shortcomings.

Development of concrete water reducing agent:
The first generation of water reducing agent: lignosulfonate (sodium, magnesium, calcium).
The second generation of water reducing agent: naphthalene sulfonate, sulfonated melamine formaldehyde, aliphatic series, amino sulfonic acid series.
The third generation of water reducing agent is: polycarboxylate superplasticizer.

RFQ:
	Q1. What is the MOQ? 
	A1: 1MT 

	Q2. Can you supply free sample? 
	A2: Yes, we can supply 1-3kg free sample. 

	Q3: Are you a manufacturer or a trading company?

	A3: We are a manufacturer with fine chemical materials manufacturer in China.
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